(form "00075" (size 45 10)
  (help "00075_TIP_0")
  (heading "DIGITISER COMMUNICATIONS")
  (label (position  4  3) (text "Port"))
  (label (position  4  4) (text "Baud"))
  (label (position  4  5) (text "Parity"))
  (label (position  4  6) (text "# Data bits"))
  (label (position  4  7) (text "# Stop bits"))
  (label (position  4  8) (text "Beep"))
  (field "port" (position 20  3) (display_length 20) (input allowed)
    (null allowed) (max_length 20))
  (field "baud" (position 20  4) (display_length  6) (input allowed)
    (value_in "50" "75" "110" "134" "150" "200" "300" "600" "1200" "1800" "2400" "4800" "9600" "19200" "38400")
    (translate lower) (null allowed) (max_length 6)
                (dependency (value "port") != "WINTAB"))
  (field "parity" (position 20  5) (display_length  6) (input allowed)
    (max_length 8)
    (value_in "none" "odd" "even")
    (translate lower) (null allowed) (max_length 4)
                (dependency (value "port") != "WINTAB"))
  (field "no_data_bits" (position 20  6) (display_length  1) (input allowed)
    (value_in "7" "8")
    (translate lower) (null allowed) (max_length 1)
                (dependency (value "port") != "WINTAB"))
  (field "no_stop_bits" (position 20  7) (display_length  1) (input allowed)
    (value_in "1" "2")
    (translate lower) (null allowed) (max_length 1)
                (dependency (value "port") != "WINTAB"))
  (field "beep" (position 20  8) (display_length  1) (input allowed)
    (value_in "Y" "N")
    (translate upper) (null allowed) (max_length 1))
  (default_buttons)
)
