(form "11118" (size 51  9)
  (heading "Edit customised firing sequence parameters")  
  (field "row_number" (position 15  7) (display_length 16) (input allowed)
    (format integer_4) (low_bound 1) (null disallowed) (max_length 32))
  (field "delay_name" (position 15  7) (display_length 16) (input allowed)
    (max_length 32) (null disallowed))  
  (field "tolerance" (position 15  7) (display_length 16) (input allowed)
    (null disallowed) (format real_8) (low_bound 0.01) (max_length 32) )  
  (field "reset_rowtime"   (position 12 13) (display_length 3) (input allowed)
    (null disallowed) (value_in "Yes" "No") (default "No"))
  (field "cumulative_delaytime" (position 15  7) (display_length 16) (input allowed)
    (dependency(value "reset_rowtime") == "Yes")(null disallowed)
    (format real_8) (low_bound 0) (max_length 32) )
  (field "current_cumulative_delaytime" (position 15  7) (display_length 16)
    (input disallowed) (format real_8) (max_length 32) )
  (default_buttons)
)
