(form "00386" (position 2 2) (size 76 22)
  (help "00386_TIP_0")  
  (heading "INCONSISTENT BACKSIGHT/SETUP STATION COMBINATION")

  (label (position  2 3) (text "Backsight station"))
  (field "backsight" (position 24  3) (display_length  16) (input disallowed)
   (null disallowed))

  (label (position  2 4) (text "Setup station"))
  (field "setup" (position 24  4) (display_length  16) (input disallowed)
   (null disallowed))

  (label (position  2 6) 
    (text "The Backsight station may not be a suitable backsight for the Setup station."))

  (label (position  2 7) 
    (text "Backsight/Setup stations are deemed suitable provided the entry in the station_fr"))

  (label (position  2 8) 
    (text "field of either the Backsight or Setup stations define a "))

  (label (position  2 9) 
    (text "connection between the 2 stations."))

  (label (position  2 11) 
    (text "If this connection exists, the reverse bearing can be obtained from the stored"))

  (label (position  2 12) 
    (text "value in the database."))

  (label (position  2 14) 
    (text "You may either:"))

  (label (position  2 15) 
    (text "a) Choose APPLY and accept a reverse bearing by calculating a value using"))

  (label (position  2 16) 
    (text "the Backsight and Setup station co-ordinates."))

  (label (position  2 18) 
    (text "b) Choose CANCEL and abort the calculation of co-ordinates until the problem"))

  (label (position  2 19) 
    (text "with the survey is resolved."))

  (default_buttons)
)
