(form "00387" (size 76 18)
  (heading "INCONSISTENT DATABASE REVERSE BEARING VALUE")

  (label (position  2 3) (text "Backsight station"))
  (field "backsight" (position 24  3) (display_length  16) (input disallowed)
   (null disallowed))

  (label (position  2 4) (text "Setup station"))
  (field "setup" (position 24  4) (display_length  16) (input disallowed)
   (null disallowed))

  (label (position  2 6) (text "Stored bearing"))
  (field "stored_bearing" (position 20  6) (display_length  10)
    (format dms_angle) (input disallowed) (decimals 4))

  (label (position  35 6) (text "Calculated bearing"))
  (field "calculated_bearing" (position 50  6) (display_length  10)
    (format dms_angle) (input disallowed) (decimals 4))

  (label (position  2 7) 
    (text "The stored bearing obtained from the database for the line from the Setup station to the"))

  (label (position  2 8) 
    (text "Backsight station differs by greater than 2 minutes from the calculated reverse bearing."))

  (label (position  2 10) 
    (text "You must choose which action to take before continuing with co-ordinate calculations."))

  (menu (position 2 13) (size 22  4)
    (grid  1  4)
    (item (function "use stored bearing") (text "Use stored bearing"))
    (item (function "use calculated bearing") (text "Use Calculated bearing"))
    (item (function "help") (text "Help"))
    (item (function "cancel") (text "Cancel"))
  )
  (label (position  2 12) (foreground (user_option "form_text_highlight"))
    (text "Press the required button"))

  (label (position  26 13) 
    (text "Obtain the reverse bearing from the rev_brng field."))

  (label (position  26 14) 
    (text "Calculate the reverse bearing using the station co-ordinates"))

  (label (position  26 16) 
    (text "Cancel this function and don't save the results."))
)
